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This specification section is provided in CSI-format, and intended to be included in the Project Manual for a construction project.  Delete models and options not required for your project, and modify to your project requirements.


SECTION 102814

BABY CHANGING STATIONS

GENERAL

SECTION INCLUDES


Baby Changing Stations, Matte Black:
0. Elite Series, surface-mounted vertical design. (Koala Model KB311-SSWM-MBLK)


RELATED REQUIREMENTS

Section 061000 - Rough Carpentry, blocking in walls.

Section 092100 - Plaster and Gypsum Board Assemblies, blocking in walls.

Section 093000 - Tiling, coordination with tile layout and installation.

SUBMITTALS

Product Data:  Submit manufacturer's data sheets for each product specified, including the following.
0. Installation instructions and recommendations, including templates and rough-in measurements.
0. Storage and handling requirements and recommendations.
0. Cleaning and maintenance instructions.

QUALITY ASSURANCE

Manufacturer:  Provide products manufactured by a company with a minimum of 5 years successful experience manufacturing similar products.

Single Source Requirements:  To the greatest extent possible provide products from a single manufacturer.

Accessibility Requirements:  Comply with requirements applicable in the jurisdiction of the project, including but not limited to ADA, ICC A117.1, International Building Code (IBC), and state building code requirements as applicable.

Baby Changing Stations:  Provide products which comply with the following standards and requirements.
0. Antimicrobial Treatment:  Changing surfaces embedded with Microban®, with antibacterial claim substantiated by Kirby-Bauer test or other manufacturer approved equivalent standard industry test methodology.
0. Americans with Disabilities Act (ADA). 
0. ICC A117.1 - Accessible and Usable Building and Facilities.
0. ANSI  Z535.4 - Product Safety Signs and Labels. 
0. ASTM F2285 - Standard Consumer Safety Performance Specification for Diaper Changing Tables for Commercial Use. 
0. ASTM G 21 - Standard Practice for Determining Resistance of Synthetic Polymeric Materials to Fungi.
0. European Standards:  EN 12221 Changing units for domestic use.
0. CPSIA: Conformity with the U.S. Consumer Product Safety Commission (CPSC) product safety rules, bans, standards and regulations that include applicable chemical compliance requirements.

Manufacturing Location:  United States.

DELIVERY, STORAGE, AND HANDLING

Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations.  Protect from damage.

WARRANTY 

Manufacturer’s Warranties:  Submit manufacturer’s standard 5-year limited warranty for materials and workmanship and include a provision for replacement caused by vandalism.


PRODUCTS

MANUFACTURER

Basis of Design Products: Based on the quality and performance requirements of the project, specifications are based solely on the products of Koala Kare Products, a Division of Bobrick, www.koalakare.com.  Location of manufacturing shall be the United States.

Substitutions:  The Architect will consider products of comparable manufacturers as a substitution, pending the contractor's submission of adequate documentation of the substitution in accordance with procedures in Division 1 of the Project Manual.  Documentation shall include a list of five similar projects of equivalent size where products have been installed for a minimum of two years, and manufacturer's certification that products are fabricated in the United States.


BABY CHANGING STATIONS, MATTE BLACK 

A. Surface-Mounted Vertical Design Matte Black Baby Changing Station:
0. Basis of Design:  Elite Series model KB311-SSWM-MBLK with external matte black bag hook as manufactured by Koala Kare Products, a Division of Bobrick.
0. Handle: Replaceable aluminum handle with matte black finish, positioned to permit operation of the changing station with less than 5 lbs. of force

0. Front Panel: One-piece, seamless, deep-drawn 18-8, Type 304, 20-gauge (0.91 mm) stainless steel with matte black finish, rounded corners, and laser-etched logo.
0. Flange: One-piece, seamless, deep-drawn 18-8, Type 304, 18-gauge (1.2 mm) stainless steel with matte black finish. Flange edges and corners shall have radii that complement the arcs of the front panel.
0. Skirt: Constructed of Type 304, 20-gauge (0.91 mm) stainless steel with matte black finish. Skirt corners shall have radii that complement the arcs of the front panel.
0. Steel Frame: Concealed 11-gauge steel chassis frame comprising integral 1" diameter steel tubing that supports the changing bed and interfaces with an 11-gauge steel wall-mounting bracket to provide a steel-on-steel hinge stop. The wall frame shall serve as the wall-mounting bracket.
0. External Diaper Bag Hook: 18-8, Type 304, 3/4 inch (19mm) diameter, wall-mounted, solid stainless steel rod with matte black finish. 
0. Dual Dispensers: Two integrated dispensers for sanitary bed liners and Koala Diaper Pouch® disposal bags. Equipped with a tumbler lock keyed alike with Bobrick restroom accessories.
0. Aesthetics: Unit shall have no plastic covering or visible plastic on the front of the unit and no adhesive labels applied to the front panel. 
0. Bed Surface: injection-molded polypropylene with Microban® antimicrobial additive, tested for efficacy in accordance with ISO 22196.
0. Surface is contoured, concave and smooth. Bed surface shall be minimum 535 sq. in.
0. Performance: Unit has minimal deflection from 90 degrees with a 150-lb. static load placed in the center of the changing surface. Unit exceeds ASTM Standard F2285 static load requirement of 100 lbs.
0. Complies with requirements applicable in the jurisdiction of the project, including but not limited to ADA, ICC A117.1, International Building Code (IBC), and state building code requirements as applicable. Also complies with ASTM Standard F2285, Standard Consumer Safety Performance Specification for Diaper Changing Stations for Commercial use and EN 12221 for changing units for domestic use.
0. Operation: Concealed gas shock providing controlled opening and closing of the changing station bed.
0. Instruction Graphics:  Universal instruction graphics and safety messages in multiple languages.
0. Safety Straps:  Replaceable safety strap. 

EXECUTION

INSTALLATION

Install products in strict compliance with manufacturer’s written instructions and recommendations, including the following:
0. Verify wall blocking has been installed properly.
0. Verify wall location does not interfere with door swings or use of fixtures.
0. Use fasteners and anchors suitable for wall substrate and project conditions.
0. Install units at location and height indicated on the Drawings.
0. Install units level, plumb and in proper relationship with adjacent construction.
0. Adjust for proper operation.

PROTECTION

Protect installed products until completion of project.

Touch-up, repair or replace damaged products before Substantial Completion.
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